; Installation inf for the SEC SOC USB Bulk IO Test B/D

[Version]
Signature="$CHICAGO$"
Class=USB
ClassGUID={36FC9E60-C465-11CF-8056-444553540000}
provider=%ProviderName%
DriverVer=08/05/1999

[SourceDisksNames]
1="USB Downloader Installation Disk for SEC SOC",,,

[SourceDisksFiles]
SECBULK.sys = 1
SECBULK.inf = 1

[Manufacturer]
%MfgName%=SystemLsi

[SystemLsi]
%USB\VID_5345&PID_1234.DeviceDesc%=SECBULK.Dev, USB\VID_5345&PID_1234

;[PreCopySection]
;HKR,,NoSetupUI,,1

[DestinationDirs]
SECBULK.Files.Ext = 10,System32\Drivers
SECBULK.Files.Inf = 10,INF

[SECBULK.Dev]
CopyFiles=SECBULK.Files.Ext, SECBULK.Files.Inf
AddReg=SECBULK.AddReg

[SECBULK.Dev.NT]
CopyFiles=SECBULK.Files.Ext, SECBULK.Files.Inf
AddReg=SECBULK.AddReg

[SECBULK.Dev.NT.Services]
Addservice = SECBULK, 0x00000002, SECBULK.AddService

[SECBULK.AddService]
DisplayName    = %SECBULK.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\SECBULK.sys
LoadOrderGroup = Base

[SECBULK.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,SECBULK.sys
HKLM,"System\Currentcontrolset\Services\SecBulk\Parameters","MaximumTransferSize",0x10001,4096
HKLM,"System\Currentcontrolset\Services\SecBulk\Parameters","DebugLevel",0x10001,2


[SECBULK.Files.Ext]
SECBULK.sys

[SECBULK.Files.Inf]
SECBULK.Inf


;---------------------------------------------------------------;

[Strings]
ProviderName="purnnamu"
MfgName="SEC, SYSTEM LSI"
USB\VID_5345&PID_1234.DeviceDesc="SEC SOC Test Board"
SECBULK.SvcDesc="SECBULK.sys, SEC SOC USBD Driver"

